*LIGO Laboratory / LIGO Scientific Collaboration*

LIGO- E1200416-v2 Advanced LIGO 6/14/2012

TwinCAT Library for Demdodulators

Daniel Sigg

Distribution of this document:

LIGO Scientific Collaboration

This is an internal working note  
of the LIGO Laboratory.

|  |  |
| --- | --- |
| **California Institute of Technology**  **LIGO Project – MS 18-34**  **1200 E. California Blvd.**  **Pasadena, CA 91125**  Phone (626) 395-2129  Fax (626) 304-9834  E-mail: info@ligo.caltech.edu | **Massachusetts Institute of Technology**  **LIGO Project – NW22-295**  **185 Albany St**  **Cambridge, MA 02139**  Phone (617) 253-4824  Fax (617) 253-7014  E-mail: info@ligo.mit.edu |
| **LIGO Hanford Observatory**  **P.O. Box 159**  **Richland WA 99352**  Phone 509-372-8106  Fax 509-372-8137 | **LIGO Livingston Observatory**  **P.O. Box 940**  **Livingston, LA 70754**  Phone 225-686-3100  Fax 225-686-7189 |

http://www.ligo.caltech.edu/

|  |  |
| --- | --- |
| **Library** | |
| Title | Demodulator |
| Version | 2 |
| TwinCAT version | 2.11 |
| Name space | Demodulator |
| Author | Daniel Sigg |
| Description | Monitors the 4-channel demodulator, [D0902796](https://dcc.ligo.org/cgi-bin/private/DocDB/ShowDocument?docid=7742), the 2-channel demodulator, [D1000181](https://dcc.ligo.org/cgi-bin/private/DocDB/ShowDocument?docid=8795), and the 2-channel phase-frequency discriminator, [D1002476](https://dcc.ligo.org/cgi-bin/private/DocDB/ShowDocument?docid=21102).  Demodulators are used by ISC for length and alignment sensing, whereas phase-frequency demodulators are used for laser locking. Each channels comes with an RF monitor of the LO and the RF inputs. The 2-channel chassis implement an additional power supply monitor, which indicates that the supply voltages are within range. Each channel of the phase-frequency discriminator has a monitor of the sign of the frequency comparison.  The RF detector measures the power off a -20 dB directional coupler. It is a logarithmic device and has the following equation:  LO:  RF:  The 4-channel demodulator chassis used for ASC has the LO split between all channels, whereas the LO for the LSC is per channel. |
| Error codes | 1 – Power supply voltages out-of-range  2 – LO power level out-of-range  3 – RF power level overload  4 – Sign is wrong |
| Library dependencies | Error |

|  |  |
| --- | --- |
| **Demodulator Type**  TYPE DemodulatorTypeEnum :  (Quad, Single, SingleFast, PhaseFrequency);  END\_TYPE | |
| Type name | DemodulatorTypeEnum |
| Description | Enumerates the different types of available demodulators |
| Definition | ENUM |
| Element | Name: Quad  Description: Denotes an ASC quad demodulator chassis used for wavefront sensing |
| Element | Name: Single  Description: Denotes a single channel of an LSC quad demodulator chassis used for length sensing |
| Element | Name: SingleFast  Description: Denotes a single channel of a fast LSC dual demodulator chassis used for length sensing |
| Element | Name: PhaseFrequency  Description: Denotes a single channel of an LSC dual phase-frequency discriminator chassis used for laser locking |

|  |  |
| --- | --- |
| **Hardware Input Type**  TYPE DemodulatorInStruct :  STRUCT  RFMon: INT;  LOMon: INT;  Sign: BOOL;  PowerOk: BOOL;  END\_STRUCT  END\_TYPE | |
| Type name | DemodulatorInStruct |
| Description | Structure of the hardware inputs that are wired up for a demodulator channel. The phase-frequency discriminator only uses the sign. The 2-channel chassis share a power ok bit. The power ok bit is reflected in the hardware output structure. The second channel daisy chains its power ok input from the output of the first channel. |
| Definition | STRUCT |
| Element | Name: RFMon  Type: INT  Description: Monitors the RF power at the RF input |
| Element | Name: LOMon  Type: INT  Description: Monitors the RF power at the LO input |
| Element | Name: Sign  Type: BOOL  Description: Sign of phase-frequency discriminator |
| Element | Name: PowerOk  Type: BOOL  Description: Voltage monitor readback |

|  |  |
| --- | --- |
| **Hardware Input Type**  TYPE DemodulatorQuadInStruct:  STRUCT  Seg: ARRAY [1..4] OF DemodulatorInStruct;  END\_STRUCT  END\_TYPE | |
| Type name | DemodulatorQuadInStruct |
| Description | An array of four DemodulatorInStruct used to describe a four channel demodulator chassis used for wavefront sensing |
| Definition | STRUCT |
| Element | Name: Seg  Type: ARRAY [1..4] OF DemodulatorInStruct  Description: Quad array of demodulator channels |

|  |  |
| --- | --- |
| **Hardware Output Type**  TYPE DemodulatorOutStruct :  STRUCT  PowerOk: BOOL;  END\_STRUCT  END\_TYPE | |
| Type name | DemodulatorOutStruct |
| Description | Structure of the hardware outputs that are wired up for a demodulator channel. The power ok bit is a simple reflection of the power ok bit at the input. It is used for daisy chaining multiple channels. |
| Definition | STRUCT |
| Element | Name: PowerOk  Type: BOOL  Description: Voltage monitor readback |

|  |  |
| --- | --- |
| **User Interface Type**  TYPE DemodulatorLscStruct :  STRUCT  Error: ErrorStruct;  DemodulatorType: DemodulatorTypeEnum;  RFMon: LREAL;  RFMax: LREAL;  LOMon: LREAL;  LONom: LREAL;  Sign: BOOL;  SignNom: BOOL;  PowerOk: BOOL;  END\_STRUCT  END\_TYPE | |
| Type name | DemodulatorLscStruct |
| Description | Structure of the user interface tags that are used to control a single channel of a demodulator or a phase-frequency discriminator |
| Definition | STRUCT |
| Output Tag | Name: Error  Type: ErrorStruct  Description: For error handler |
| Output Tag | Name: DemodulatorType  Type: DemodulatorTypeEnum  Description: Demotes the type of demodulator or phase-frequency discriminator channel |
| Output Tag | Name: RFMon  Type: LREAL  Description: Monitors the RF power at the RF input in dBm |
| Input Tag | Name: RFMax  Type: LREAL  Description: Maximum value for the RF power at the RF input in dBm |
| Output Tag | Name: LOMon  Type: LREAL  Description: Monitors the RF power at the LO input in dBm |
| Input Tag | Name: LONom  Type: LREAL  Description: Nominal value for the RF power at the LO input in dBm |
| Output Tag | Name: Sign  Type: BOOL  Description: Monitors the sign of a phase-frequency discriminator |
| Input Tag | Name: SignNom  Type: LREAL  Description: Nominal value for the sign of a phase-frequency discriminator |
| Output Tag | Name: PowerOk  Type: BOOL  Description: Voltage monitor readback |

|  |  |
| --- | --- |
| **User Interface Type**  TYPE DemodulatorAscStruct :  STRUCT  Error: ErrorStruct;  RFMon: ARRAY [1..4] OF LREAL;  RFMax: LREAL;  LOMonChannel: ARRAY [1..4] OF LREAL;  LOMon: LREAL;  LONom: LREAL;  END\_STRUCT  END\_TYPE | |
| Type name | DemodulatorAscStruct |
| Description | Structure of the user interface tags that are used to control a four channel demodulator chassis used for wavefront sensing |
| Definition | STRUCT |
| Output Tag | Name: Error  Type: ErrorStruct  Description: For error handler |
| Output Tag | Name: RFMon  Type: ARRAY [1..4] OF LREAL  Description: Monitors the RF power at each RF input in dBm |
| Input Tag | Name: RFMax  Type: LREAL  Description: Maximum value for the RF power at the RF inputs in dBm |
| Output Tag | Name: LOMonChannel  Type: LREAL  Description: RF power at each of the LO inputs in dBm |
| Output Tag | Name: LOMon  Type: LREAL  Description: RF power at the LO input in dBm (sum of all channels) |
| Input Tag | Name: LONom  Type: LREAL  Description: Nominal value for the RF power at the LO input in dBm |

|  |  |
| --- | --- |
| **Function Block**  FUNCTION\_BLOCK DemodulatorLscFB  VAR\_INPUT  DemdulatorType: DemodulatorTypeEnum;  DemdulatorIn: DemdulatorInStruct;  END\_VAR  VAR\_OUTPUT  DemdulatorOut: DemdulatorOutStruct;  END\_VAR  VAR\_IN\_OUT  DemdulatorLsc: DemdulatorLscStruct;  END\_VAR  VAR  END\_VAR | |
| Name | DemodulatorLscFB |
| Description | Controls a single channel of a demodulator or phase-frequency discriminator chassis. One function block for each demodulator channel needs to be instantiated. |
| Input argument | Name: DemdulatorType  Type: DemodulatorTypeEnum  Description: Defines the used demodulator chassis |
| Input argument | Name: DemdulatorIn  Type: DemdulatorInStruct  Description: Input hardware structure |
| Output argument | Name: DemdulatorOut  Type: DemdulatorOutStruct  Description: Output hardware structure |
| In/out argument | Name: DemdulatorLsc  Type: DemdulatorLscStruct  Description: User Interface structure |

|  |  |
| --- | --- |
| **Function Block**  FUNCTION\_BLOCK DemodulatorAscFB  VAR\_INPUT  DemdulatorIn: DemodulatorQuadInArray;  END\_VAR  VAR\_IN\_OUT  DemdulatorAsc: DemdulatorAscStruct;  END\_VAR  VAR  END\_VAR | |
| Name | DemodulatorAscFB |
| Description | Controls a quad channel demodulator chassis. One function block for each ASC demodulator chassis needs to be instantiated. |
| Input argument | Name: DemdulatorIn  Type: DemodulatorQuadInStruct  Description: Input hardware structure |
| In/out argument | Name: DemdulatorAsc  Type: DemdulatorAscStruct  Description: User Interface structure |

|  |  |
| --- | --- |
| **Visual** | |
| Name | DemodulatorAscVis |
| Description | Displays RF Max and Mon, LO Mon and Nom, power status, sign status, and error status |
| Placeholder | Name: DemodulatorAsc  Type: DemodulatorAscStruct  Description: Asc Demodulator structure |

|  |  |
| --- | --- |
| **Visual** | |
| Name | DemodulatorLscPhaseFrequencyVis |
| Description | Displays RF Max and Mon, LO Mon and Nom, power status, sign status, and error status |
| Placeholder | Name: DemodulatorLsc  Type: DemodulatorLscStruct  Description: Phase frequency Lsc Demodulator structure |

|  |  |
| --- | --- |
| **Visual** | |
| Name | DemodulatorLscQuadVis |
| Description | Displays RF Max and Mon, LO Mon and Nom, and error status |
| Placeholder | Name: DemodulatorLsc  Type: DemodulatorLscStruct  Description: Quad Lsc Demodulator structure |

|  |  |
| --- | --- |
| **Visual** | |
| Name | DemodulatorLscSingleVis |
| Description | Displays RF Max and Mon, LO Mon and Nom, and error status |
| Placeholder | Name: DemodulatorLsc  Type: DemodulatorLscStruct  Description: Single Lsc Demodulator structure |

|  |  |
| --- | --- |
| **Visual** | |
| Name | DemodulatorLscSingleFastVis |
| Description | Displays RF Max and Mon, LO Mon and Nom, power status, and error status |
| Placeholder | Name: DemodulatorLsc  Type: DemodulatorLscStruct  Description: Single Fast Lsc Demodulator structure |