Title: ISC Dewhitening Board
Drawing Number: D2500133
Revision: 1
Author: Daniel Sigg
Board Size: 8.440" x 7.000"
Layers: 6
Smallest feature: 10mil
Components: both sides

Manufacturing instructions:
- Preferably use 1oz. copper weight
- Board thickness: approximately 62 mils

Assembly instructions:
- Solder large plastic capacitors by hand, lay down to minimize height

Layer Stack (top to bottom):
isc_dewhitening_filter.GTL
isc_dewhitening_filter.GP1
isc_dewhitening_filter.G1
isc_dewhitening_filter.GP2
isc_dewhitening_filter.GP3
isc_dewhitening_filter.GBL

Silkscreen (top/bottom):
isc_dewhitening_filter.GTO
isc_dewhitening_filter.GBO

Solder Mask (top/bottom):
isc_dewhitening_filter.GTS
isc_dewhitening_filter.GBS

Paste Mask (top/bottom):
isc_dewhitening_filter.GTP
isc_dewhitening_filter.GBP

Board Outline:
isc_dewhitening_filter.GM

Drill File:
isc_dewhitening_filter.txt

Pick and Place:
Pick Place for isc_dewhitening_filter.txt

ODB+ Files:
isc_dewhitening_filter.zip
